|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747Phone: 310-243-3000 • Office: 310-243-3171 www.csudh.edu/ehs |

|  |  |  |
| --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Pressure Washing |
|  | **Name of Shop or Dept:** | CSUDH Campus - Maintenance |
| **Job Title(s):** |  |
| **Analyzed by:** | M. Williams |
| **Date:** | 10/1/2021 |
| **Required PPE:** |
|

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Slip-Resistant Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Mask/Face Protection** |
| http://i.pgcdn.com/pi/78/99/15/789915284_260.jpg | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600 | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | Nuisance Removal Dust Mask, PK 50 |
| [x]  | [x]  | [ ]  | [x]  | [x]  | [ ]  |

 |
| **Required/Recommended Trainings:** |
|  |
| **TASK** | **HAZARDS** | **CONTROLS** |
| Pressure washing with a Hotsy or Landa Washer | **Slips****Trips****Falls****Lacerations****Struck-by****Electrocution** | **Don** booties and place wet floor signs in direct area before operating a pressure washer.**Use** a safety vest when there is risk of vehicular traffic in the area.**Safety** glasses shall be worn to prevent particles from flying up and coming in contact with eyes.**Be** familiar with how to turn off machine and bleed pressure out before operating the equipment.**Make** sure electrical connections are grounded using a 3-prong outlet.**Keep** water spray away from electric wiring or electric shock may result.**Always** hold the spray gun with both hands to prevent kick back.**Firmly** grip spray gun before starting to prevent gun from whipping and causing bodily harm.**Never** spray washer towards persons or vehicles as it can cause bodily harm.**Do not** attempt to overreach or stand on an unstable footing while operating equipment.**Never** leave equipment unattended. |