|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | **Injury & Illness Prevention Program**  Job Safety Analysis Form | | |
| 1000 E Victoria St.• Carson, CA 90747 Phone: 310-243-3000 • Office: 310-243-3171  [www.csudh.edu/ehs](http://www.csudh.edu/ehs) | | |
|  | | | | |
| **Picture of task/equipment:** | **Task:** | | Dumping waste with Vestil JMD-1000 | |
|  | **Name of Shop**  **or Dept:** | | CSUDH Campus - Sustainability | |
| **Job Title(s):** | | Sustainability, Mover | |
| **Analyzed by:** | | M. Williams | |
| **Date:** | | 5/11/2022 | |
| **Required PPE:** | | | | |
| **Work Boots Gloves Hearing Protection Safety Glasses Safety Vest Mask/Face Protection**  Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902  Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110  ☒ ☐ ☐ ☒ ☐ ☐ | | | | |
| **Required/Recommended Trainings:** | | | | |
| **IIPP Equipment Specific** | | | | |
| **TASK** | **HAZARDS** | | | **CONTROLS** |
| Dumping waste in the Vestil JMD-1000 tote dumper | Struck By’s Pinch Lacerations | | | D Inspect the tote for damage before each lift. Do not attempt to pick up the tote unless it is in good condition.  D Always have the floor lock engaged solidly with the floor surface when the dumper is in operation.  D Lock wheels before operation  D Verify that the tote is engaged and held securely by the dumper before proceeding to raise the tote.  D Always watch the dumper and the tote carefully when the dumper is in operation.  D Stand away from the side of the dumper when it is in operation. Stay clear of any potential pinch and shear points.  D Be alert to the possibility of splashing or flying material when dumping loads.  D Do not use the dumper if any damage or unusual noise is observed.  D When moving the dumper for charging, raise handlebar and push dumper to charging station  D Ensure wheels are locked when charging |