|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747Phone: 310-243-3000 • Office: 310-243-3171 www.csudh.edu/ehs |

|  |  |  |
| --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Operating a Street Sweeper |
|  | **Name of Shop or Dept:** | CSUDH Campus -  |
| **Job Title(s):** |  |
| **Analyzed by:** | M. Williams |
| **Date:** | 10/1/2021 |
| **Required PPE:** |
|

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Work Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Dust Mask** |
| Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600 | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | Nuisance Removal Dust Mask, PK 50 |
| [ ]  | [ ]  | [ ]  | [x]  | [ ]  | [x]  |

 |
| **Required/Recommended Trainings:** |
| User must train with supervisor | User must read owner’s manual | User must have valid driver’s license |
| **TASK** | **HAZARDS** | **CONTROLS** |
| **Inspect** the sweeper before each use.**Must** only be used out of doors**Seatbelt** must be worn | **Eye Injury from particles****Respiratory irritation from inhalation of Dust****Traffic Hazard**  | **Equipment** to be Inspected after each use**Equipment** to be Serviced bi-annually by factory representative. |