|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**  Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747  Phone: 310-243-3000 • Office: 310-243-3171  www.csudh.edu/ehs |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Operating a Street Sweeper | | |
|  | **Name of Shop or Dept:** | CSUDH Campus - | | |
| **Job Title(s):** |  | | |
| **Analyzed by:** | M. Williams | | |
| **Date:** | 10/1/2021 | | |
| **Required PPE:** | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | **Work Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Dust Mask** | | Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | [http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600](javascript:swapimage('http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600')) | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | [Nuisance Removal Dust Mask, PK 50](javascript:%20void(0)) | |  |  |  |  |  |  | | | | | |
| **Required/Recommended Trainings:** | | | | |
| User must train with supervisor | User must read owner’s manual | | | User must have valid driver’s license |
| **TASK** | **HAZARDS** | | **CONTROLS** | |
| **Inspect** the sweeper before each use.  **Must** only be used out of doors  **Seatbelt** must be worn | **Eye Injury from particles**  **Respiratory irritation from inhalation of Dust**  **Traffic Hazard** | | **Equipment** to be Inspected after each use  **Equipment** to be Serviced bi-annually by factory representative. | |