|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747Phone: 310-243-3000 • Office: 310-243-3171 www.csudh.edu/ehs |

|  |  |  |
| --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Weed Trimmer |
| Groundskeeper Tools 083007  Photos 010 | **Name of Shop or Dept:** | CSUDH Campus - Grounds |
| **Job Title(s):** | Groundskeepers |
| **Analyzed by:** | M. Williams |
| **Date:** | 10/1/2021 |
| **Required PPE:** |
|

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Work Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Mask/Face Protection** |
| Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600 | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | Nuisance Removal Dust Mask, PK 50 |
| [x]  | [x]  | [x]  | [x]  | [x]  | [x]  |

 |
| **Required/Recommended Trainings:** |
| Slip, Trip, Fall Safety | Equipment Safety Precautions |
| **TASK** | **HAZARDS** | **CONTROLS** |
| Operating a gas-poweredweed trimmer**Groundskeeper Tools 083007  Photos 012** | **Struck By’s****Lacerations****Slips****Trips****Falls****Vapor** **Inhalation****Fire** | **Don** PPE before starting equipment, including non-slip work boots, Gloves, Hearing **Protection**, Safety glasses, a mask and a safety vest (when working near public roadways).**Wear** long pants, as flying debris can come in contact with lower limbs.**Make** sure all guards are in place before operating equipment.**Inspect** spark plug cap and lead to make sure they are not damaged, otherwise electric shock can occur.**Do not** operate within 50ft of persons or traffic as injury or ricochet can occur.**Do not** operate next to glass, such as windows.**Watch** for uneven surfaces, holes and slopes; take extra care with footing to avoid STF’s.**Keep** hands, arms and dry debris away from the muffler, it can result in burns or fires.**Never** start the equipment indoors as exhaust can create a harmful breathing atmosphere.**Hold** trimmer head just above ground and let the cord cut; never force the cutter into grass or weeds.**Do not** try to make adjustments to the cutting cord while the machine is on.**Do not** try to remove debris while the machine is in operation; make sure machine is off before clearing. |